TOOL	3350638976
CFID	98
CMOD	2
SKEY	rowinski
STRE
	SGLB	354044
		STRE
			SORD	0
				CLAS	354008
			ESBR
		ESTR
	ESBR
	SGLB	354539
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	General/Initialize
			ESBR
			SGLB	SignalP/Input
			ESBR
		ESTR
	ESBR
	SGLB	354540
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	General/Initialize
			ESBR
			SGLB	SignalP/Trigger
			ESBR
		ESTR
	ESBR
	SGLB	354580
		STRE
			SORD	0
				CSYM	354580
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
		ESTR
	ESBR
	SGLB	354579
		STRE
			SORD	0
				CSYM	354579
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354009
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	General/Initialize
			ESBR
		ESTR
	ESBR
	SGLB	354008
		STRE
			SORD	0
				CSYM	354009
			ESBR
			SGLB	General/Initialize
			ESBR
			SGLB	Hierarchy/Attach Conn
			ESBR
			SGLB	Hierarchy/Remove Conn
			ESBR
		ESTR
	ESBR
	SGLB	354725
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354724
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354723
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354722
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354721
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354720
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354719
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354718
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354717
		STRE
			SORD	0
				CLAS	354008
			ESBR
		ESTR
	ESBR
	SGLB	354716
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354715
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354714
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354713
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354712
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354711
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354578
		STRE
			SORD	0
				CSYM	354578
			ESBR
			SGLB	Drive/Source Tag	/3u;
				LITO	1
			ESBR
			SGLB	Drive/Get Source Tag	/2u;
				LITO	1
			ESBR
			SGLB	Drive/Destination Tag	/3u;
				LITO	2
			ESBR
			SGLB	Drive/Get Destination Tag	/2u;
				LITO	2
			ESBR
		ESTR
	ESBR
	SGLB	354764
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354763
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354762
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354761
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354760
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354759
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354758
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354757
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354756
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354755
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354754
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354765
		STRE
			SORD	0
				CLAS	354580
			ESBR
		ESTR
	ESBR
	SGLB	354753
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354752
		STRE
			SORD	0
				CLAS	354580
			ESBR
		ESTR
	ESBR
	SGLB	354751
		STRE
			SORD	0
				CLAS	354580
			ESBR
		ESTR
	ESBR
	SGLB	354750
		STRE
			SORD	0
				CLAS	354580
			ESBR
		ESTR
	ESBR
	SGLB	354747
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354746
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354745
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354744
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354743
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354742
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354741
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354749
		STRE
			SORD	0
				CLAS	354580
			ESBR
		ESTR
	ESBR
	SGLB	354739
		STRE
			SORD	0
				CLAS	354580
			ESBR
		ESTR
	ESBR
	SGLB	354732
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354731
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354730
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354729
		STRE
			SORD	0
				CLAS	354579
			ESBR
		ESTR
	ESBR
	SGLB	354570
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/INPUT	/3v,-300,300,-300,300;Enter INPUT (%)...
				LITO	1
			ESBR
			SGLB	Drive/Get INPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/THRESHOLD (>)	/3v,-300,300,-300,300;Enter THRESHOLD (>) (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get THRESHOLD (>)	/2v,-300,300,-300,300;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/OFFSET	/3v,-300,300,-300,300;Enter OFFSET (%)...
				LITO	3
			ESBR
			SGLB	Drive/Get OFFSET	/2v,-300,300,-300,300;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/MODULUS	/3t,FALSE,TRUE;Enter MODULUS...
				LITO	4
			ESBR
			SGLB	Drive/Get MODULUS	/2t,FALSE,TRUE;
				LITO	4
			ESBR
			SGLB	Drive/INVERT	/3t,FALSE,TRUE;Enter INVERT...
				LITO	5
			ESBR
			SGLB	Drive/Get INVERT	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/Get DIGOUT	/2t,FALSE,TRUE;
				LITO	6
			ESBR
		ESTR
	ESBR
	SGLB	354740
		STRE
			SORD	0
				CLAS	354570
			ESBR
		ESTR
	ESBR
	SGLB	354748
		STRE
			SORD	0
				CLAS	354570
			ESBR
		ESTR
	ESBR
	SGLB	354603
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get DIGIN ENABLE	/2t,FALSE,TRUE;
				LITO	1
			ESBR
		ESTR
	ESBR
	SGLB	354738
		STRE
			SORD	0
				CLAS	354603
			ESBR
		ESTR
	ESBR
	SGLB	354737
		STRE
			SORD	0
				CLAS	354603
			ESBR
		ESTR
	ESBR
	SGLB	354736
		STRE
			SORD	0
				CLAS	354569
			ESBR
		ESTR
	ESBR
	SGLB	354735
		STRE
			SORD	0
				CLAS	354743
			ESBR
		ESTR
	ESBR
	SGLB	354734
		STRE
			SORD	0
				CLAS	354569
			ESBR
		ESTR
	ESBR
	SGLB	354569
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/OUTPUT	/3v,-300,300,-300,300;Enter OUTPUT (%)...
				LITO	1
			ESBR
			SGLB	Drive/Get OUTPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/VALUE FOR TRUE	/3v,-300,300,-300,300;Enter VALUE FOR TRUE (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get VALUE FOR TRUE	/2v,-300,300,-300,300;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/VALUE FOR FALSE	/3v,-300,300,-300,300;Enter VALUE FOR FALSE (%)...
				LITO	3
			ESBR
			SGLB	Drive/Get VALUE FOR FALSE	/2v,-300,300,-300,300;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/Get RAW INPUT	/2t,FALSE,TRUE;
				LITO	4
			ESBR
		ESTR
	ESBR
	SGLB	354568
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/INPUT	/3v,-300,300,-300,300;Enter INPUT (%)...
				LITO	1
			ESBR
			SGLB	Drive/Get INPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/% TO GET 10V	/3v,-300,300,-300,300;Enter % TO GET 10V (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get % TO GET 10V	/2v,-300,300,-300,300;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/OFFSET	/3v,-300,300,-300,300;Enter OFFSET (%)...
				LITO	3
			ESBR
			SGLB	Drive/Get OFFSET	/2v,-300,300,-300,300;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/CALIBRATION	/3v,-200,200,-200,200;Enter CALIBRATION (%)...
				LITO	4
			ESBR
			SGLB	Drive/Get CALIBRATION	/2v,-200,200,-200,200;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/MODULUS	/3t,DISABLED,ENABLED;Enter MODULUS...
				LITO	5
			ESBR
			SGLB	Drive/Get MODULUS	/2t,DISABLED,ENABLED;
				LITO	5
			ESBR
			SGLB	Drive/Get ANALOG OUTPUT	/2v,-10,10,-10,10;%.3fV;
				LITO	6
			ESBR
		ESTR
	ESBR
	SGLB	354733
		STRE
			SORD	0
				CLAS	354568
			ESBR
		ESTR
	ESBR
	SGLB	354728
		STRE
			SORD	0
				CLAS	354567
			ESBR
		ESTR
	ESBR
	SGLB	354727
		STRE
			SORD	0
				CLAS	354580
			ESBR
		ESTR
	ESBR
	SGLB	354726
		STRE
			SORD	0
				CLAS	354567
			ESBR
		ESTR
	ESBR
	SGLB	354567
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get SCALED INPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/CALIBRATION	/3v,-300,300,-300,300;Enter CALIBRATION (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get CALIBRATION	/2v,-300,300,-300,300;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/OFFSET	/3v,-100,100,-100,100;Enter OFFSET (%)...
				LITO	3
			ESBR
			SGLB	Drive/Get OFFSET	/2v,-100,100,-100,100;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/MAX VALUE	/3v,-300,300,-300,300;Enter MAX VALUE (%)...
				LITO	4
			ESBR
			SGLB	Drive/Get MAX VALUE	/2v,-300,300,-300,300;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/MIN VALUE	/3v,-300,300,-300,300;Enter MIN VALUE (%)...
				LITO	5
			ESBR
			SGLB	Drive/Get MIN VALUE	/2v,-300,300,-300,300;%.2f%%;
				LITO	5
			ESBR
			SGLB	Drive/Get RAW INPUT	/2v,-10,10,-10,10;%.3fV;
				LITO	6
			ESBR
		ESTR
	ESBR
	SGLB	354559
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/RUN STOP TIME	/3v,-1000,1000,0,1000;Enter RUN STOP TIME (Secs)...
				LITO	1
			ESBR
			SGLB	Drive/Get RUN STOP TIME	/2v,-1000,1000,0,1000;%.1fs;
				LITO	1
			ESBR
			SGLB	Drive/RUN STOP LIMIT	/3v,-1000,1000,0,1000;Enter RUN STOP LIMIT (Secs)...
				LITO	2
			ESBR
			SGLB	Drive/Get RUN STOP LIMIT	/2v,-1000,1000,0,1000;%.1fs;
				LITO	2
			ESBR
			SGLB	Drive/FAST STOP TIME	/3v,-1000,1000,0,1000;Enter FAST STOP TIME (Secs)...
				LITO	3
			ESBR
			SGLB	Drive/Get FAST STOP TIME	/2v,-1000,1000,0,1000;%.1fs;
				LITO	3
			ESBR
			SGLB	Drive/FAST STOP LIMIT	/3v,-1000,1000,0,1000;Enter FAST STOP LIMIT (Secs)...
				LITO	4
			ESBR
			SGLB	Drive/Get FAST STOP LIMIT	/2v,-1000,1000,0,1000;%.1fs;
				LITO	4
			ESBR
			SGLB	Drive/USE SYSTEM RAMP	/3t,FALSE,TRUE;Enter USE SYSTEM RAMP...
				LITO	5
			ESBR
			SGLB	Drive/Get USE SYSTEM RAMP	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/PRE-START DELAY	/3v,-30,30,0,30;Enter PRE-START DELAY (Secs)...
				LITO	6
			ESBR
			SGLB	Drive/Get PRE-START DELAY	/2v,-30,30,0,30;%.3fs;
				LITO	6
			ESBR
			SGLB	Drive/READY DELAY	/3v,-30,30,0,30;Enter READY DELAY (Secs)...
				LITO	7
			ESBR
			SGLB	Drive/Get READY DELAY	/2v,-30,30,0,30;%.3fs;
				LITO	7
			ESBR
			SGLB	Drive/CONTACTOR DELAY	/3v,-1000,1000,0,1000;Enter CONTACTOR DELAY (Secs)...
				LITO	8
			ESBR
			SGLB	Drive/Get CONTACTOR DELAY	/2v,-1000,1000,0,1000;%.1fs;
				LITO	8
			ESBR
			SGLB	Drive/STOP ZERO SPEED	/3v,-120,120,0,100;Enter STOP ZERO SPEED (%)...
				LITO	9
			ESBR
			SGLB	Drive/Get STOP ZERO SPEED	/2v,-120,120,0,100;%.2f%%;
				LITO	9
			ESBR
			SGLB	Drive/PROG STOP I-LIM	/3v,-150,150,0,150;Enter PROG STOP I-LIM (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get PROG STOP I-LIM	/2v,-150,150,0,150;%.2f%%;
				LITO	10
			ESBR
		ESTR
	ESBR
	SGLB	354571
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get DRIVE START	/2t,FALSE,TRUE;
				LITO	1
			ESBR
			SGLB	Drive/Get DRIVE ENABLE	/2t,FALSE,TRUE;
				LITO	2
			ESBR
			SGLB	Drive/Get OPERATING MODE	/2e,INITIALIZE,COAST STOP,PROGRAM STOP,AUTOTUNE,RUN,JOG,RAMPED STOP,RUN NORMAL STOP,JOG NORMAL STOP,PRE START 1,PRE START 2,STOPPED;
				LITO	3
			ESBR
			SGLB	Drive/Get RUN	/2t,FALSE,TRUE;
				LITO	4
			ESBR
			SGLB	Drive/Get COAST STOP	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/Get PROGRAM STOP	/2t,FALSE,TRUE;
				LITO	6
			ESBR
			SGLB	Drive/Get SEQ RUN INPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	7
			ESBR
			SGLB	Drive/Get SEQ OUTPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/AUX START	/3t,FALSE,TRUE;Enter AUX START...
				LITO	9
			ESBR
			SGLB	Drive/Get AUX START	/2t,FALSE,TRUE;
				LITO	9
			ESBR
			SGLB	Drive/AUX JOG	/3t,FALSE,TRUE;Enter AUX JOG...
				LITO	10
			ESBR
			SGLB	Drive/Get AUX JOG	/2t,FALSE,TRUE;
				LITO	10
			ESBR
			SGLB	Drive/AUX ENABLE	/3t,FALSE,TRUE;Enter AUX ENABLE...
				LITO	11
			ESBR
			SGLB	Drive/Get AUX ENABLE	/2t,FALSE,TRUE;
				LITO	11
			ESBR
			SGLB	Drive/START	/3t,FALSE,TRUE;Enter START...
				LITO	12
			ESBR
			SGLB	Drive/Get START	/2t,FALSE,TRUE;
				LITO	12
			ESBR
			SGLB	Drive/JOG INPUT	/3t,FALSE,TRUE;Enter JOG INPUT...
				LITO	13
			ESBR
			SGLB	Drive/Get JOG INPUT	/2t,FALSE,TRUE;
				LITO	13
			ESBR
			SGLB	Drive/ENABLE	/3t,FALSE,TRUE;Enter ENABLE...
				LITO	14
			ESBR
			SGLB	Drive/Get ENABLE	/2t,FALSE,TRUE;
				LITO	14
			ESBR
		ESTR
	ESBR
	SGLB	354561
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/REFSPEED	/3v,-200,200,-200,200;Enter REFSPEED (%)...
				LITO	1
			ESBR
			SGLB	Drive/Get REFSPEED	/2v,-200,200,-200,200;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/MAX SPEED RPM	/3v,-6000,6000,0,6000;Enter MAX SPEED RPM (RPM)...
				LITO	2
			ESBR
			SGLB	Drive/Get MAX SPEED RPM	/2v,-6000,6000,0,6000;%.0fRPM;
				LITO	2
			ESBR
			SGLB	Drive/ENCODER LINES	/3u,0,8000;Enter ENCODER LINES...
				LITO	3
			ESBR
			SGLB	Drive/Get ENCODER LINES	/2u,0,8000;
				LITO	3
			ESBR
			SGLB	Drive/OFFSET	/3v,-30000,30000,-30000,30000;Enter OFFSET...
				LITO	4
			ESBR
			SGLB	Drive/Get OFFSET	/2v,-30000,30000,-30000,30000;%.0f;
				LITO	4
			ESBR
			SGLB	Drive/OFFSET SCALE	/3u,0,1000;Enter OFFSET SCALE...
				LITO	5
			ESBR
			SGLB	Drive/Get OFFSET SCALE	/2u,0,1000;
				LITO	5
			ESBR
			SGLB	Drive/RESET	/3t,FALSE,TRUE;Enter RESET...
				LITO	6
			ESBR
			SGLB	Drive/Get RESET	/2t,FALSE,TRUE;
				LITO	6
			ESBR
			SGLB	Drive/POS CALC ENABLE	/3t,FALSE,TRUE;Enter POS CALC ENABLE...
				LITO	7
			ESBR
			SGLB	Drive/Get POS CALC ENABLE	/2t,FALSE,TRUE;
				LITO	7
			ESBR
			SGLB	Drive/POSITION ERROR	/3v,-30000,30000,-30000,30000;Enter POSITION ERROR...
				LITO	8
			ESBR
			SGLB	Drive/Get POSITION ERROR	/2v,-30000,30000,-30000,30000;%.0f;
				LITO	8
			ESBR
			SGLB	Drive/MAX POSITION ERR	/3v,-300,300,-300,300;Enter MAX POSITION ERR...
				LITO	9
			ESBR
			SGLB	Drive/Get MAX POSITION ERR	/2v,-300,300,-300,300;%.2f;
				LITO	9
			ESBR
			SGLB	Drive/REF SCALE A	/3v,-30000,30000,-30000,30000;Enter REF SCALE A...
				LITO	10
			ESBR
			SGLB	Drive/Get REF SCALE A	/2v,-30000,30000,-30000,30000;%.0f;
				LITO	10
			ESBR
			SGLB	Drive/REF SCALE B	/3v,-30000,30000,-30000,30000;Enter REF SCALE B...
				LITO	11
			ESBR
			SGLB	Drive/Get REF SCALE B	/2v,-30000,30000,-30000,30000;%.0f;
				LITO	11
			ESBR
			SGLB	Drive/REF ENCODER I/P	/3v,-30000,30000,-30000,30000;Enter REF ENCODER I/P...
				LITO	12
			ESBR
			SGLB	Drive/Get REF ENCODER I/P	/2v,-30000,30000,-30000,30000;%.0f;
				LITO	12
			ESBR
			SGLB	Drive/Get SATURATED	/2t,FALSE,TRUE;
				LITO	13
			ESBR
			SGLB	Drive/Get OVERFLOW	/2t,FALSE,TRUE;
				LITO	14
			ESBR
			SGLB	Drive/INCH ADVANCE	/3t,FALSE,TRUE;Enter INCH ADVANCE...
				LITO	15
			ESBR
			SGLB	Drive/Get INCH ADVANCE	/2t,FALSE,TRUE;
				LITO	15
			ESBR
			SGLB	Drive/INCH RETARD	/3t,FALSE,TRUE;Enter INCH RETARD...
				LITO	16
			ESBR
			SGLB	Drive/Get INCH RETARD	/2t,FALSE,TRUE;
				LITO	16
			ESBR
			SGLB	Drive/INCH RATE	/3v,-1000,1000,0,1000;Enter INCH RATE...
				LITO	17
			ESBR
			SGLB	Drive/Get INCH RATE	/2v,-1000,1000,0,1000;%.1f;
				LITO	17
			ESBR
		ESTR
	ESBR
	SGLB	354576
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/SETPT. RATIO	/3v,-3,3,-3,3;Enter SETPT. RATIO...
				LITO	1
			ESBR
			SGLB	Drive/Get SETPT. RATIO	/2v,-3,3,-3,3;%.4f;
				LITO	1
			ESBR
			SGLB	Drive/SETPT. SIGN	/3t,NEG,POS;Enter SETPT. SIGN...
				LITO	2
			ESBR
			SGLB	Drive/Get SETPT. SIGN	/2t,NEG,POS;
				LITO	2
			ESBR
			SGLB	Drive/SCALED INPUT	/3v,-300,300,-300,300;Enter SCALED INPUT (%)...
				LITO	3
			ESBR
			SGLB	Drive/Get SCALED INPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/RAW INPUT	/3v,-300,300,-300,300;Enter RAW INPUT (%)...
				LITO	4
			ESBR
			SGLB	Drive/Get RAW INPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/OUTPUT	/3v,-300,300,-300,300;Enter OUTPUT (%)...
				LITO	5
			ESBR
			SGLB	Drive/Get OUTPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	5
			ESBR
		ESTR
	ESBR
	SGLB	354564
		STRE
			SORD	0
				CLAS	354540
			ESBR
			SGLB	Drive/P3 MODE	/3e,OPTION BOARD,5703 MASTER,5703 SLAVE,TAG LIST VT100,TAG LIST NEWPORT,REMOTE MMI,BUSY,BUSY,BUSY,BUSY;Enter P3 MODE...
				LITO	1
			ESBR
			SGLB	Drive/Get P3 MODE	/2e,OPTION BOARD,5703 MASTER,5703 SLAVE,TAG LIST VT100,TAG LIST NEWPORT,REMOTE MMI,BUSY,BUSY,BUSY,BUSY;
				LITO	1
			ESBR
			SGLB	Drive/P3 BAUD RATE	/3e,300,600,1200,4800,19920,38400,57600;Enter P3 BAUD RATE...
				LITO	2
			ESBR
			SGLB	Drive/Get P3 BAUD RATE	/2e,300,600,1200,4800,19920,38400,57600;
				LITO	2
			ESBR
			SGLB	Drive/TAG 1	/3u,0,600;Enter TAG 1...
				LITO	3
			ESBR
			SGLB	Drive/Get TAG 1	/2u,0,600;
				LITO	3
			ESBR
			SGLB	Drive/TAG 2	/3u,0,600;Enter TAG 2...
				LITO	4
			ESBR
			SGLB	Drive/Get TAG 2	/2u,0,600;
				LITO	4
			ESBR
			SGLB	Drive/TAG 3	/3u,0,600;Enter TAG 3...
				LITO	5
			ESBR
			SGLB	Drive/Get TAG 3	/2u,0,600;
				LITO	5
			ESBR
			SGLB	Drive/TAG 4	/3u,0,600;Enter TAG 4...
				LITO	6
			ESBR
			SGLB	Drive/Get TAG 4	/2u,0,600;
				LITO	6
			ESBR
			SGLB	Drive/TAG 5	/3u,0,600;Enter TAG 5...
				LITO	7
			ESBR
			SGLB	Drive/Get TAG 5	/2u,0,600;
				LITO	7
			ESBR
			SGLB	Drive/FULL TAG LIST	/3t,FALSE,TRUE;Enter FULL TAG LIST...
				LITO	8
			ESBR
			SGLB	Drive/Get FULL TAG LIST	/2t,FALSE,TRUE;
				LITO	8
			ESBR
		ESTR
	ESBR
	SGLB	354630
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/KIMR_INT	/3u,0,32000;Enter KIMR_INT...
				LITO	1
			ESBR
			SGLB	Drive/Get KIMR_INT	/2u,0,32000;
				LITO	1
			ESBR
			SGLB	Drive/AUTO RAMP INCRMT	/3u,1,50;Enter AUTO RAMP INCRMT...
				LITO	2
			ESBR
			SGLB	Drive/Get AUTO RAMP INCRMT	/2u,1,50;
				LITO	2
			ESBR
			SGLB	Drive/LINK V FILT GAIN	/3u,0,32000;Enter LINK V FILT GAIN...
				LITO	3
			ESBR
			SGLB	Drive/Get LINK V FILT GAIN	/2u,0,32000;
				LITO	3
			ESBR
			SGLB	Drive/TERM V FILT GAIN	/3u,0,32000;Enter TERM V FILT GAIN...
				LITO	4
			ESBR
			SGLB	Drive/Get TERM V FILT GAIN	/2u,0,32000;
				LITO	4
			ESBR
			SGLB	Drive/TERM V FLTGN DSP	/3u,0,32000;Enter TERM V FLTGN DSP...
				LITO	5
			ESBR
			SGLB	Drive/Get TERM V FLTGN DSP	/2u,0,32000;
				LITO	5
			ESBR
			SGLB	Drive/Get AUTOCAL MAX RPM	/2v,-30000,30000,0,30000;%.0fRPM;
				LITO	6
			ESBR
			SGLB	Drive/LOAD FACTOR @BS	/3v,-100,100,50,100;Enter LOAD FACTOR @BS (%)...
				LITO	7
			ESBR
			SGLB	Drive/Get LOAD FACTOR @BS	/2v,-100,100,50,100;%.1f%%;
				LITO	7
			ESBR
			SGLB	Drive/LOAD FACTOR @2BS	/3v,-100,100,50,100;Enter LOAD FACTOR @2BS (%)...
				LITO	8
			ESBR
			SGLB	Drive/Get LOAD FACTOR @2BS	/2v,-100,100,50,100;%.1f%%;
				LITO	8
			ESBR
			SGLB	Drive/MIN LINK V RATIO	/3v,-100,100,50,100;Enter MIN LINK V RATIO (%)...
				LITO	9
			ESBR
			SGLB	Drive/Get MIN LINK V RATIO	/2v,-100,100,50,100;%.2f%%;
				LITO	9
			ESBR
			SGLB	Drive/AUTOCAL MAX RPM	/3v,-30000,30000,0,30000;Enter AUTOCAL MAX RPM (RPM)...
				LITO	10
			ESBR
			SGLB	Drive/Get AUTOCAL MAX RPM	/2v,-30000,30000,0,30000;%.0fRPM;
				LITO	10
			ESBR
		ESTR
	ESBR
	SGLB	354629
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get SET DRIVE RATING	/2e,USER,0.75kW,1.1kW,1.5kW,2.2kW,4kW,5.5kW,7.5kW,11kW,15kW,18.5kW,22kW,30kW,37kW,45kW,55kW,75kW;
				LITO	1
			ESBR
			SGLB	Drive/MAG I AUTOTUNE	/3t,FALSE,TRUE;Enter MAG I AUTOTUNE...
				LITO	2
			ESBR
			SGLB	Drive/Get MAG I AUTOTUNE	/2t,FALSE,TRUE;
				LITO	2
			ESBR
			SGLB	Drive/SET Tr < RTD SPD	/3t,FALSE,TRUE;Enter SET Tr < RTD SPD...
				LITO	3
			ESBR
			SGLB	Drive/Get SET Tr < RTD SPD	/2t,FALSE,TRUE;
				LITO	3
			ESBR
			SGLB	Drive/Get MAG CURRENT %	/2v,-90,90,0,90;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/Get ROTOR TIME CONST	/2v,-3000,3000,12.8,3000;%.1fms;
				LITO	5
			ESBR
			SGLB	Drive/AUTOTUNE FLAG	/3t,FALSE,TRUE;Enter AUTOTUNE FLAG...
				LITO	6
			ESBR
			SGLB	Drive/Get AUTOTUNE FLAG	/2t,FALSE,TRUE;
				LITO	6
			ESBR
			SGLB	Drive/PARAMETER SAVE	/3t,ABORT,SAVE;Enter PARAMETER SAVE...
				LITO	7
			ESBR
			SGLB	Drive/Get PARAMETER SAVE	/2t,UP TO ACTION,WORKING;
				LITO	7
			ESBR
		ESTR
	ESBR
	SGLB	354572
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/JOG SPEED 1	/3v,-100,100,-100,100;Enter JOG SPEED 1 (%)...
				LITO	1
			ESBR
			SGLB	Drive/Get JOG SPEED 1	/2v,-100,100,-100,100;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/JOG SPEED 2	/3v,-100,100,-100,100;Enter JOG SPEED 2 (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get JOG SPEED 2	/2v,-100,100,-100,100;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/MODE	/3t,FALSE,TRUE;Enter MODE...
				LITO	3
			ESBR
			SGLB	Drive/Get MODE	/2t,FALSE,TRUE;
				LITO	3
			ESBR
			SGLB	Drive/JOG ACCEL RATE	/3v,-100,100,0,100;Enter JOG ACCEL RATE (Secs)...
				LITO	4
			ESBR
			SGLB	Drive/Get JOG ACCEL RATE	/2v,-100,100,0,100;%.1fs;
				LITO	4
			ESBR
			SGLB	Drive/JOG DECEL RATE	/3v,-100,100,0,100;Enter JOG DECEL RATE (Secs)...
				LITO	5
			ESBR
			SGLB	Drive/Get JOG DECEL RATE	/2v,-100,100,0,100;%.1fs;
				LITO	5
			ESBR
		ESTR
	ESBR
	SGLB	354554
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get HEALTHY	/2t,FALSE,TRUE;
				LITO	1
			ESBR
			SGLB	Drive/Get HEALTH OUTPUT	/2t,FALSE,TRUE;
				LITO	2
			ESBR
			SGLB	Drive/Get READY	/2t,FALSE,TRUE;
				LITO	3
			ESBR
			SGLB	Drive/Get MOTOR TEMP	/2v,-200,200,-200,200;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/Get STALL TRIP	/2t,OK,ACTIVE;
				LITO	5
			ESBR
			SGLB	Drive/EXTERNAL TRIP	/3t,FALSE,TRUE;Enter EXTERNAL TRIP...
				LITO	6
			ESBR
			SGLB	Drive/Get EXTERNAL TRIP	/2t,FALSE,TRUE;
				LITO	6
			ESBR
			SGLB	Drive/MOTOR TMP.TRIP	/3v,-200,200,0,200;Enter MOTOR TMP.TRIP (%)...
				LITO	7
			ESBR
			SGLB	Drive/Get MOTOR TMP.TRIP	/2v,-200,200,0,200;%.2f%%;
				LITO	7
			ESBR
			SGLB	Drive/MOTOR TMP.RST.	/3v,-200,200,0,200;Enter MOTOR TMP.RST. (%)...
				LITO	8
			ESBR
			SGLB	Drive/Get MOTOR TMP.RST.	/2v,-200,200,0,200;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/MOTR.TMP.INHIBIT	/3t,FALSE,TRUE;Enter MOTR.TMP.INHIBIT...
				LITO	9
			ESBR
			SGLB	Drive/Get MOTR.TMP.INHIBIT	/2t,FALSE,TRUE;
				LITO	9
			ESBR
			SGLB	Drive/HEATSINK LEVEL	/3v,-200,200,0,200;Enter HEATSINK LEVEL (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get HEATSINK LEVEL	/2v,-200,200,0,200;%.2f%%;
				LITO	10
			ESBR
			SGLB	Drive/ACK ALARM	/3t,FALSE,TRUE;Enter ACK ALARM...
				LITO	11
			ESBR
			SGLB	Drive/Get ACK ALARM	/2t,FALSE,TRUE;
				LITO	11
			ESBR
			SGLB	Drive/STALL INHIBIT	/3t,FALSE,TRUE;Enter STALL INHIBIT...
				LITO	12
			ESBR
			SGLB	Drive/Get STALL INHIBIT	/2t,FALSE,TRUE;
				LITO	12
			ESBR
			SGLB	Drive/STALL TORQUE	/3v,-200,200,0,200;Enter STALL TORQUE (%)...
				LITO	13
			ESBR
			SGLB	Drive/Get STALL TORQUE	/2v,-200,200,0,200;%.2f%%;
				LITO	13
			ESBR
			SGLB	Drive/STALL SPEED	/3v,-200,200,0,200;Enter STALL SPEED (%)...
				LITO	14
			ESBR
			SGLB	Drive/Get STALL SPEED	/2v,-200,200,0,200;%.2f%%;
				LITO	14
			ESBR
			SGLB	Drive/STALL DELAY	/3v,-300,300,0,300;Enter STALL DELAY...
				LITO	15
			ESBR
			SGLB	Drive/Get STALL DELAY	/2v,-300,300,0,300;%.2f;
				LITO	15
			ESBR
			SGLB	Drive/OVER SPD INHIBIT	/3t,FALSE,TRUE;Enter OVER SPD INHIBIT...
				LITO	16
			ESBR
			SGLB	Drive/Get OVER SPD INHIBIT	/2t,FALSE,TRUE;
				LITO	16
			ESBR
			SGLB	Drive/OVER SPEED LEVEL	/3v,-200,200,0,200;Enter OVER SPEED LEVEL (%)...
				LITO	17
			ESBR
			SGLB	Drive/Get OVER SPEED LEVEL	/2v,-200,200,0,200;%.2f%%;
				LITO	17
			ESBR
			SGLB	Drive/5703 RCV.INHIBIT	/3t,FALSE,TRUE;Enter 5703 RCV.INHIBIT...
				LITO	18
			ESBR
			SGLB	Drive/Get 5703 RCV.INHIBIT	/2t,FALSE,TRUE;
				LITO	18
			ESBR
			SGLB	Drive/HEALTH STORE	/3x;Enter HEALTH STORE...
				LITO	19
			ESBR
			SGLB	Drive/Get HEALTH STORE	/2x;0x%4.4X;
				LITO	19
			ESBR
			SGLB	Drive/HEALTH WORD	/3x;Enter HEALTH WORD...
				LITO	20
			ESBR
			SGLB	Drive/Get HEALTH WORD	/2x;0x%4.4X;
				LITO	20
			ESBR
			SGLB	Drive/FIRST ALARM	/3x;Enter FIRST ALARM...
				LITO	21
			ESBR
			SGLB	Drive/Get FIRST ALARM	/2x;0x%4.4X;
				LITO	21
			ESBR
			SGLB	Drive/HEALTH INHIBIT	/3x;Enter HEALTH INHIBIT...
				LITO	22
			ESBR
			SGLB	Drive/Get HEALTH INHIBIT	/2x;0x%4.4X;
				LITO	22
			ESBR
		ESTR
	ESBR
	SGLB	354573
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get RAISE/LOWER O/P	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/RESET VALUE	/3v,-100,100,-100,100;Enter RESET VALUE (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get RESET VALUE	/2v,-100,100,-100,100;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/RAMP RATE	/3v,-600,600,0.1,600;Enter RAMP RATE (Secs)...
				LITO	3
			ESBR
			SGLB	Drive/Get RAMP RATE	/2v,-600,600,0.1,600;%.1fs;
				LITO	3
			ESBR
			SGLB	Drive/RAISE INPUT	/3t,FALSE,TRUE;Enter RAISE INPUT...
				LITO	4
			ESBR
			SGLB	Drive/Get RAISE INPUT	/2t,FALSE,TRUE;
				LITO	4
			ESBR
			SGLB	Drive/LOWER INPUT	/3t,FALSE,TRUE;Enter LOWER INPUT...
				LITO	5
			ESBR
			SGLB	Drive/Get LOWER INPUT	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/MIN VALUE	/3v,-300,300,-300,300;Enter MIN VALUE (%)...
				LITO	6
			ESBR
			SGLB	Drive/Get MIN VALUE	/2v,-300,300,-300,300;%.2f%%;
				LITO	6
			ESBR
			SGLB	Drive/MAX VALUE	/3v,-300,300,-300,300;Enter MAX VALUE (%)...
				LITO	7
			ESBR
			SGLB	Drive/Get MAX VALUE	/2v,-300,300,-300,300;%.2f%%;
				LITO	7
			ESBR
			SGLB	Drive/EXTERNAL RESET	/3t,FALSE,TRUE;Enter EXTERNAL RESET...
				LITO	8
			ESBR
			SGLB	Drive/Get EXTERNAL RESET	/2t,FALSE,TRUE;
				LITO	8
			ESBR
		ESTR
	ESBR
	SGLB	354566
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get RAMP OUTPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/RAMP ACCEL TIME	/3v,-600,600,0,600;Enter RAMP ACCEL TIME (Secs)...
				LITO	2
			ESBR
			SGLB	Drive/Get RAMP ACCEL TIME	/2v,-600,600,0,600;%.1fs;
				LITO	2
			ESBR
			SGLB	Drive/RAMP DECEL TIME	/3v,-600,600,0,600;Enter RAMP DECEL TIME (Secs)...
				LITO	3
			ESBR
			SGLB	Drive/Get RAMP DECEL TIME	/2v,-600,600,0,600;%.1fs;
				LITO	3
			ESBR
			SGLB	Drive/RAMP QUENCH	/3t,FALSE,TRUE;Enter RAMP QUENCH...
				LITO	4
			ESBR
			SGLB	Drive/Get RAMP QUENCH	/2t,FALSE,TRUE;
				LITO	4
			ESBR
			SGLB	Drive/RAMP HOLD	/3t,FALSE,TRUE;Enter RAMP HOLD...
				LITO	5
			ESBR
			SGLB	Drive/Get RAMP HOLD	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/RAMP INPUT	/3v,-100,100,-100,100;Enter RAMP INPUT (%)...
				LITO	6
			ESBR
			SGLB	Drive/Get RAMP INPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	6
			ESBR
			SGLB	Drive/% S-RAMP	/3v,-100,100,-100,100;Enter % S-RAMP (%)...
				LITO	7
			ESBR
			SGLB	Drive/Get % S-RAMP	/2v,-100,100,-100,100;%.2f%%;
				LITO	7
			ESBR
			SGLB	Drive/RAMPING THRESH.	/3v,-100,100,-100,100;Enter RAMPING THRESH. (%)...
				LITO	8
			ESBR
			SGLB	Drive/Get RAMPING THRESH.	/2v,-100,100,-100,100;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/AUTO RESET	/3t,FALSE,TRUE;Enter AUTO RESET...
				LITO	9
			ESBR
			SGLB	Drive/Get AUTO RESET	/2t,FALSE,TRUE;
				LITO	9
			ESBR
			SGLB	Drive/EXTERNAL RESET	/3t,FALSE,TRUE;Enter EXTERNAL RESET...
				LITO	10
			ESBR
			SGLB	Drive/Get EXTERNAL RESET	/2t,FALSE,TRUE;
				LITO	10
			ESBR
			SGLB	Drive/RESET VALUE	/3v,-100,100,-100,100;Enter RESET VALUE (%)...
				LITO	11
			ESBR
			SGLB	Drive/Get RESET VALUE	/2v,-100,100,-100,100;%.2f%%;
				LITO	11
			ESBR
		ESTR
	ESBR
	SGLB	354608
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/SETPOINT	/3v,-100,100,0,100;Enter SETPOINT (%)...
				LITO	1
			ESBR
			SGLB	Drive/Get SETPOINT	/2v,-100,100,0,100;%.1f%%;
				LITO	1
			ESBR
			SGLB	Drive/SETPOINT	/3v,-100,100,0,100;Enter SETPOINT (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get SETPOINT	/2v,-100,100,0,100;%.1f%%;
				LITO	2
			ESBR
			SGLB	Drive/REV DIRECTION	/3t,FALSE,TRUE;Enter REV DIRECTION...
				LITO	3
			ESBR
			SGLB	Drive/Get REV DIRECTION	/2t,FALSE,TRUE;
				LITO	3
			ESBR
			SGLB	Drive/PROGRAM	/3t,FALSE,TRUE;Enter PROGRAM...
				LITO	4
			ESBR
			SGLB	Drive/Get PROGRAM	/2t,FALSE,TRUE;
				LITO	4
			ESBR
			SGLB	Drive/LOCAL	/3t,FALSE,TRUE;Enter LOCAL...
				LITO	5
			ESBR
			SGLB	Drive/Get LOCAL	/2t,FALSE,TRUE;
				LITO	5
			ESBR
		ESTR
	ESBR
	SGLB	354553
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get RAMP OUTPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/Get RAMPING	/2t,FALSE,TRUE;
				LITO	2
			ESBR
			SGLB	Drive/RAMP ACCEL TIME	/3v,-600,600,0,600;Enter RAMP ACCEL TIME (Secs)...
				LITO	3
			ESBR
			SGLB	Drive/Get RAMP ACCEL TIME	/2v,-600,600,0,600;%.1fs;
				LITO	3
			ESBR
			SGLB	Drive/RAMP DECEL TIME	/3v,-600,600,0,600;Enter RAMP DECEL TIME (Secs)...
				LITO	4
			ESBR
			SGLB	Drive/Get RAMP DECEL TIME	/2v,-600,600,0,600;%.1fs;
				LITO	4
			ESBR
			SGLB	Drive/RAMP QUENCH	/3t,FALSE,TRUE;Enter RAMP QUENCH...
				LITO	5
			ESBR
			SGLB	Drive/Get RAMP QUENCH	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/RAMP HOLD	/3t,FALSE,TRUE;Enter RAMP HOLD...
				LITO	6
			ESBR
			SGLB	Drive/Get RAMP HOLD	/2t,FALSE,TRUE;
				LITO	6
			ESBR
			SGLB	Drive/RAMP INPUT	/3v,-100,100,-100,100;Enter RAMP INPUT (%)...
				LITO	7
			ESBR
			SGLB	Drive/Get RAMP INPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	7
			ESBR
			SGLB	Drive/% S-RAMP	/3v,-100,100,-100,100;Enter % S-RAMP (%)...
				LITO	8
			ESBR
			SGLB	Drive/Get % S-RAMP	/2v,-100,100,-100,100;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/RAMPING THRESH.	/3v,-100,100,0,100;Enter RAMPING THRESH. (%)...
				LITO	9
			ESBR
			SGLB	Drive/Get RAMPING THRESH.	/2v,-100,100,0,100;%.2f%%;
				LITO	9
			ESBR
			SGLB	Drive/AUTO RESET	/3t,FALSE,TRUE;Enter AUTO RESET...
				LITO	10
			ESBR
			SGLB	Drive/Get AUTO RESET	/2t,FALSE,TRUE;
				LITO	10
			ESBR
			SGLB	Drive/EXTERNAL RESET	/3t,FALSE,TRUE;Enter EXTERNAL RESET...
				LITO	11
			ESBR
			SGLB	Drive/Get EXTERNAL RESET	/2t,FALSE,TRUE;
				LITO	11
			ESBR
			SGLB	Drive/RESET VALUE	/3v,-100,100,-100,100;Enter RESET VALUE (%)...
				LITO	12
			ESBR
			SGLB	Drive/Get RESET VALUE	/2v,-100,100,-100,100;%.2f%%;
				LITO	12
			ESBR
		ESTR
	ESBR
	SGLB	354606
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/% LOAD @BASE SPD	/3v,-10,10,0,10;Enter % LOAD @BASE SPD (%)...
				LITO	1
			ESBR
			SGLB	Drive/Get % LOAD @BASE SPD	/2v,-10,10,0,10;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/TVolts INT RANGE	/3v,-80,80,0,80;Enter TVolts INT RANGE (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get TVolts INT RANGE	/2v,-80,80,0,80;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/SPD @ TV INT =0	/3v,-100,100,10,100;Enter SPD @ TV INT =0 (%)...
				LITO	3
			ESBR
			SGLB	Drive/Get SPD @ TV INT =0	/2v,-100,100,10,100;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/IQ @TV INTGN=MIN	/3v,-150,150,10,150;Enter IQ @TV INTGN=MIN (%)...
				LITO	4
			ESBR
			SGLB	Drive/Get IQ @TV INTGN=MIN	/2v,-150,150,10,150;%.1f%%;
				LITO	4
			ESBR
			SGLB	Drive/IQ @TV INTGN=MAX	/3v,-300,300,150,300;Enter IQ @TV INTGN=MAX (%)...
				LITO	5
			ESBR
			SGLB	Drive/Get IQ @TV INTGN=MAX	/2v,-300,300,150,300;%.1f%%;
				LITO	5
			ESBR
			SGLB	Drive/LOOP RESPNSE=nTr	/3v,-30000,30000,4,30000;Enter LOOP RESPNSE=nTr...
				LITO	6
			ESBR
			SGLB	Drive/Get LOOP RESPNSE=nTr	/2v,-30000,30000,4,30000;%.0f;
				LITO	6
			ESBR
			SGLB	Drive/FAST RESPONSE %	/3v,-115,115,100,115;Enter FAST RESPONSE % (%)...
				LITO	7
			ESBR
			SGLB	Drive/Get FAST RESPONSE %	/2v,-115,115,100,115;%.2f%%;
				LITO	7
			ESBR
		ESTR
	ESBR
	SGLB	354565
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get MAG I SCALE 0	/2v,-100,100,100,100;%.1f%%;
				LITO	1
			ESBR
			SGLB	Drive/Get MAG I SCALE 1	/2v,-100,100,0,100;%.1f%%;
				LITO	2
			ESBR
			SGLB	Drive/Get MAG I SCALE 2	/2v,-100,100,0,100;%.1f%%;
				LITO	3
			ESBR
			SGLB	Drive/Get MAG I SCALE 3	/2v,-100,100,0,100;%.1f%%;
				LITO	4
			ESBR
			SGLB	Drive/Get MAG I SCALE 4	/2v,-100,100,0,100;%.1f%%;
				LITO	5
			ESBR
			SGLB	Drive/Get MAG I SCALE 5	/2v,-100,100,0,100;%.1f%%;
				LITO	6
			ESBR
			SGLB	Drive/Get MAG I SCALE 6	/2v,-100,100,0,100;%.1f%%;
				LITO	7
			ESBR
			SGLB	Drive/Get MAG I SCALE 7	/2v,-100,100,0,100;%.1f%%;
				LITO	8
			ESBR
			SGLB	Drive/Get MAG I SCALE 8	/2v,-100,100,0,100;%.1f%%;
				LITO	9
			ESBR
			SGLB	Drive/Get TR SCALE 0	/2v,-100,100,100,100;%.1f%%;
				LITO	10
			ESBR
			SGLB	Drive/Get TR SCALE 1	/2v,-300,300,20,300;%.1f%%;
				LITO	11
			ESBR
			SGLB	Drive/Get TR SCALE 2	/2v,-300,300,20,300;%.1f%%;
				LITO	12
			ESBR
			SGLB	Drive/Get TR SCALE 3	/2v,-300,300,20,300;%.1f%%;
				LITO	13
			ESBR
			SGLB	Drive/Get TR SCALE 4	/2v,-300,300,20,300;%.1f%%;
				LITO	14
			ESBR
			SGLB	Drive/Get TR SCALE 5	/2v,-300,300,20,300;%.1f%%;
				LITO	15
			ESBR
			SGLB	Drive/Get TR SCALE 6	/2v,-300,300,20,300;%.1f%%;
				LITO	16
			ESBR
			SGLB	Drive/Get TR SCALE 7	/2v,-300,300,20,300;%.1f%%;
				LITO	17
			ESBR
			SGLB	Drive/Get TR SCALE 8	/2v,-300,300,20,300;%.1f%%;
				LITO	18
			ESBR
		ESTR
	ESBR
	SGLB	354605
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get HOME OUTPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/HOME	/3t,FALSE,TRUE;Enter HOME...
				LITO	2
			ESBR
			SGLB	Drive/Get HOME	/2t,FALSE,TRUE;
				LITO	2
			ESBR
			SGLB	Drive/HOMING DISTANCE	/3u,0,30000;Enter HOMING DISTANCE...
				LITO	3
			ESBR
			SGLB	Drive/Get HOMING DISTANCE	/2u,0,30000;
				LITO	3
			ESBR
			SGLB	Drive/1/ENCODER SCALE	/3v,-100,100,0.01,100;Enter 1/ENCODER SCALE...
				LITO	4
			ESBR
			SGLB	Drive/Get 1/ENCODER SCALE	/2v,-100,100,0.01,100;%.2f;
				LITO	4
			ESBR
			SGLB	Drive/LINEAR  O/P	/3t,FALSE,TRUE;Enter LINEAR  O/P...
				LITO	5
			ESBR
			SGLB	Drive/Get LINEAR  O/P	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/HOME INPUT	/3v,-100,100,-100,100;Enter HOME INPUT (%)...
				LITO	6
			ESBR
			SGLB	Drive/Get HOME INPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	6
			ESBR
		ESTR
	ESBR
	SGLB	354604
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get OUTPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/Get ACCEL O/P	/2v,-150,150,0,150;%.2f;
				LITO	2
			ESBR
			SGLB	Drive/Get AT SPEED	/2t,FALSE,TRUE;
				LITO	3
			ESBR
			SGLB	Drive/INPUT	/3v,-100,100,-100,100;Enter INPUT (%)...
				LITO	4
			ESBR
			SGLB	Drive/Get INPUT	/2v,-100,100,-100,100;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/RESET	/3t,FALSE,TRUE;Enter RESET...
				LITO	5
			ESBR
			SGLB	Drive/Get RESET	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/RESET VALUE	/3v,-300,300,-300,300;Enter RESET VALUE (%)...
				LITO	6
			ESBR
			SGLB	Drive/Get RESET VALUE	/2v,-300,300,-300,300;%.2f%%;
				LITO	6
			ESBR
			SGLB	Drive/ACCELERATION	/3v,-100,100,0,100;Enter ACCELERATION...
				LITO	7
			ESBR
			SGLB	Drive/Get ACCELERATION	/2v,-100,100,0,100;%.2f;
				LITO	7
			ESBR
			SGLB	Drive/JERK	/3v,-100,100,0,100;Enter JERK...
				LITO	8
			ESBR
			SGLB	Drive/Get JERK	/2v,-100,100,0,100;%.2f;
				LITO	8
			ESBR
			SGLB	Drive/QUENCH	/3t,FALSE,TRUE;Enter QUENCH...
				LITO	9
			ESBR
			SGLB	Drive/Get QUENCH	/2t,FALSE,TRUE;
				LITO	9
			ESBR
			SGLB	Drive/AT SPEED LEVEL	/3v,-100,100,0,100;Enter AT SPEED LEVEL (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get AT SPEED LEVEL	/2v,-100,100,0,100;%.2f%%;
				LITO	10
			ESBR
			SGLB	Drive/OVERSHOOT THRESH	/3v,-100,100,0,100;Enter OVERSHOOT THRESH (%)...
				LITO	11
			ESBR
			SGLB	Drive/Get OVERSHOOT THRESH	/2v,-100,100,0,100;%.2f%%;
				LITO	11
			ESBR
		ESTR
	ESBR
	SGLB	354562
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get PRESET O/P	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/SELECT 1	/3t,FALSE,TRUE;Enter SELECT 1...
				LITO	2
			ESBR
			SGLB	Drive/Get SELECT 1	/2t,FALSE,TRUE;
				LITO	2
			ESBR
			SGLB	Drive/SELECT 2	/3t,FALSE,TRUE;Enter SELECT 2...
				LITO	3
			ESBR
			SGLB	Drive/Get SELECT 2	/2t,FALSE,TRUE;
				LITO	3
			ESBR
			SGLB	Drive/SELECT 3	/3t,FALSE,TRUE;Enter SELECT 3...
				LITO	4
			ESBR
			SGLB	Drive/Get SELECT 3	/2t,FALSE,TRUE;
				LITO	4
			ESBR
			SGLB	Drive/INPUT 1	/3v,-300,300,-300,300;Enter INPUT 1 (%)...
				LITO	5
			ESBR
			SGLB	Drive/Get INPUT 1	/2v,-300,300,-300,300;%.2f%%;
				LITO	5
			ESBR
			SGLB	Drive/SIGN	/3t,NEG,POS;Enter SIGN...
				LITO	6
			ESBR
			SGLB	Drive/Get SIGN	/2t,NEG,POS;
				LITO	6
			ESBR
			SGLB	Drive/INPUT 2	/3v,-300,300,-300,300;Enter INPUT 2 (%)...
				LITO	7
			ESBR
			SGLB	Drive/Get INPUT 2	/2v,-300,300,-300,300;%.2f%%;
				LITO	7
			ESBR
			SGLB	Drive/INPUT 3	/3v,-300,300,-300,300;Enter INPUT 3 (%)...
				LITO	8
			ESBR
			SGLB	Drive/Get INPUT 3	/2v,-300,300,-300,300;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/INPUT 4	/3v,-300,300,-300,300;Enter INPUT 4 (%)...
				LITO	9
			ESBR
			SGLB	Drive/Get INPUT 4	/2v,-300,300,-300,300;%.2f%%;
				LITO	9
			ESBR
			SGLB	Drive/INPUT 5	/3v,-300,300,-300,300;Enter INPUT 5 (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get INPUT 5	/2v,-300,300,-300,300;%.2f%%;
				LITO	10
			ESBR
			SGLB	Drive/INPUT 6	/3v,-300,300,-300,300;Enter INPUT 6 (%)...
				LITO	11
			ESBR
			SGLB	Drive/Get INPUT 6	/2v,-300,300,-300,300;%.2f%%;
				LITO	11
			ESBR
			SGLB	Drive/INPUT 7	/3v,-300,300,-300,300;Enter INPUT 7 (%)...
				LITO	12
			ESBR
			SGLB	Drive/Get INPUT 7	/2v,-300,300,-300,300;%.2f%%;
				LITO	12
			ESBR
			SGLB	Drive/INPUT 8	/3v,-300,300,-300,300;Enter INPUT 8 (%)...
				LITO	13
			ESBR
			SGLB	Drive/Get INPUT 8	/2v,-300,300,-300,300;%.2f%%;
				LITO	13
			ESBR
		ESTR
	ESBR
	SGLB	354574
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get INVERSE TIME O/P	/2v,-200,200,-150,150;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/AIMING POINT	/3v,-200,200,0,150;Enter AIMING POINT (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get AIMING POINT	/2v,-200,200,0,150;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/DELAY	/3v,-1000,1000,0,1000;Enter DELAY (Secs)...
				LITO	3
			ESBR
			SGLB	Drive/Get DELAY	/2v,-1000,1000,0,1000;%.1fs;
				LITO	3
			ESBR
			SGLB	Drive/DOWN RATE	/3v,-600,600,0,600;Enter DOWN RATE (Secs)...
				LITO	4
			ESBR
			SGLB	Drive/Get DOWN RATE	/2v,-600,600,0,600;%.1fs;
				LITO	4
			ESBR
			SGLB	Drive/UP RATE	/3v,-600,600,0,600;Enter UP RATE (Secs)...
				LITO	5
			ESBR
			SGLB	Drive/Get UP RATE	/2v,-600,600,0,600;%.1fs;
				LITO	5
			ESBR
		ESTR
	ESBR
	SGLB	354767
		STRE
			SORD	0
				CLAS	354543
			ESBR
		ESTR
	ESBR
	SGLB	354766
		STRE
			SORD	0
				CLAS	354543
			ESBR
		ESTR
	ESBR
	SGLB	354543
		STRE
			SORD	0
				CLAS	354539
			ESBR
			SGLB	Drive/Get SPT SUM O/P	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/RATIO 0	/3v,-3,3,-3,3;Enter RATIO 0...
				LITO	2
			ESBR
			SGLB	Drive/Get RATIO 0	/2v,-3,3,-3,3;%.4f;
				LITO	2
			ESBR
			SGLB	Drive/RATIO 1	/3v,-3,3,-3,3;Enter RATIO 1...
				LITO	3
			ESBR
			SGLB	Drive/Get RATIO 1	/2v,-3,3,-3,3;%.4f;
				LITO	3
			ESBR
			SGLB	Drive/SIGN 0	/3t,NEG,POS;Enter SIGN 0...
				LITO	4
			ESBR
			SGLB	Drive/Get SIGN 0	/2t,NEG,POS;
				LITO	4
			ESBR
			SGLB	Drive/SIGN 1	/3t,NEG,POS;Enter SIGN 1...
				LITO	5
			ESBR
			SGLB	Drive/Get SIGN 1	/2t,NEG,POS;
				LITO	5
			ESBR
			SGLB	Drive/DIVIDER 0	/3v,-3,3,-3,3;Enter DIVIDER 0...
				LITO	6
			ESBR
			SGLB	Drive/Get DIVIDER 0	/2v,-3,3,-3,3;%.4f;
				LITO	6
			ESBR
			SGLB	Drive/DIVIDER 1	/3v,-3,3,-3,3;Enter DIVIDER 1...
				LITO	7
			ESBR
			SGLB	Drive/Get DIVIDER 1	/2v,-3,3,-3,3;%.4f;
				LITO	7
			ESBR
			SGLB	Drive/LIMIT	/3v,-300,300,-300,300;Enter LIMIT (%)...
				LITO	8
			ESBR
			SGLB	Drive/Get LIMIT	/2v,-300,300,-300,300;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/INPUT 0	/3v,-100,100,-100,100;Enter INPUT 0 (%)...
				LITO	9
			ESBR
			SGLB	Drive/Get INPUT 0	/2v,-100,100,-100,100;%.2f%%;
				LITO	9
			ESBR
			SGLB	Drive/INPUT 1	/3v,-100,100,-100,100;Enter INPUT 1 (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get INPUT 1	/2v,-100,100,-100,100;%.2f%%;
				LITO	10
			ESBR
			SGLB	Drive/INPUT 2	/3v,-100,100,-100,100;Enter INPUT 2 (%)...
				LITO	11
			ESBR
			SGLB	Drive/Get INPUT 2	/2v,-100,100,-100,100;%.2f%%;
				LITO	11
			ESBR
		ESTR
	ESBR
	SGLB	354555
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get TOTAL SPD.DMD.	/2v,-120,120,-110,110;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/Get SPEED FB UNFIL	/2v,-120,120,-150,150;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/Get SPEED FEEDBACK	/2v,-120,120,-150,150;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/Get SPEED ERROR	/2v,-120,120,-150,150;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/Get AT ZERO SPEED	/2t,FALSE,TRUE;
				LITO	5
			ESBR
			SGLB	Drive/Get AT ZERO SETPOINT	/2t,FALSE,TRUE;
				LITO	6
			ESBR
			SGLB	Drive/Get AT STANDSTILL	/2t,FALSE,TRUE;
				LITO	7
			ESBR
			SGLB	Drive/Get SPEED SETPOINT	/2v,-120,120,-110,110;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/Get DIRECT SPT1	/2v,-120,120,-110,110;%.2f%%;
				LITO	9
			ESBR
			SGLB	Drive/Get TERMINAL VOLTS	/2v,-10000,10000,-10000,10000;%.0fV;
				LITO	10
			ESBR
			SGLB	Drive/Get DC LINK VOLTS	/2v,-1000,1000,-1000,1000;%.0fV;
				LITO	11
			ESBR
			SGLB	Drive/Get TERM V INTEGRAL	/2v,-200,200,0,200;%.2f%%;
				LITO	12
			ESBR
			SGLB	Drive/Get ENCODER	/2v,-20000,20000,-20000,20000;%.0fRPM;
				LITO	13
			ESBR
			SGLB	Drive/ENCODER SIGN	/3t,NEG,POS;Enter ENCODER SIGN...
				LITO	14
			ESBR
			SGLB	Drive/Get ENCODER SIGN	/2t,NEG,POS;
				LITO	14
			ESBR
			SGLB	Drive/SPEED FBK FILTER	/2t,FALSE,TRUE;Enter SPEED FBK FILTER...
				LITO	15
			ESBR
			SGLB	Drive/Get SPEED FBK FILTER	/2t,FALSE,TRUE;
				LITO	15
			ESBR
			SGLB	Drive/SPD. PROP. GAIN	/3v,-250,250,0,250;Enter SPD. PROP. GAIN...
				LITO	16
			ESBR
			SGLB	Drive/Get SPD. PROP. GAIN	/2v,-250,250,0,250;%.2f;
				LITO	16
			ESBR
			SGLB	Drive/SPD. INT. TIME	/3v,-30000,30000,1,30000;Enter SPD. INT. TIME (mSec)...
				LITO	17
			ESBR
			SGLB	Drive/Get SPD. INT. TIME	/2v,-30000,30000,1,30000;%.0fms;
				LITO	17
			ESBR
			SGLB	Drive/INT. DEFEAT	/3t,FALSE,TRUE;Enter INT. DEFEAT...
				LITO	18
			ESBR
			SGLB	Drive/Get INT. DEFEAT	/2t,FALSE,TRUE;
				LITO	18
			ESBR
			SGLB	Drive/DIRECT RATIO	/3v,-1,1,-1,1;Enter DIRECT RATIO...
				LITO	19
			ESBR
			SGLB	Drive/Get DIRECT RATIO	/2v,-1,1,-1,1;%.4f;
				LITO	19
			ESBR
			SGLB	Drive/DIRECT SPT. MAX	/3v,-120,120,0,100;Enter DIRECT SPT. MAX (%)...
				LITO	20
			ESBR
			SGLB	Drive/Get DIRECT SPT. MAX	/2v,-120,120,0,100;%.2f%%;
				LITO	20
			ESBR
			SGLB	Drive/DIRECT SPT. MIN	/3v,-120,120,-100,0;Enter DIRECT SPT. MIN (%)...
				LITO	21
			ESBR
			SGLB	Drive/Get DIRECT SPT. MIN	/2v,-120,120,-100,0;%.2f%%;
				LITO	21
			ESBR
			SGLB	Drive/DIRECT ENABLE	/3t,FALSE,TRUE;Enter DIRECT ENABLE...
				LITO	22
			ESBR
			SGLB	Drive/Get DIRECT ENABLE	/2t,FALSE,TRUE;
				LITO	22
			ESBR
			SGLB	Drive/MAIN SPD.SPT.	/3v,-120,120,-110,110;Enter MAIN SPD.SPT. (%)...
				LITO	23
			ESBR
			SGLB	Drive/Get MAIN SPD.SPT.	/2v,-120,120,-110,110;%.2f%%;
				LITO	23
			ESBR
			SGLB	Drive/MAX SPEED	/3v,-120,120,0,110;Enter MAX SPEED (%)...
				LITO	24
			ESBR
			SGLB	Drive/Get MAX SPEED	/2v,-120,120,0,110;%.2f%%;
				LITO	24
			ESBR
			SGLB	Drive/MIN SPEED	/3v,-120,120,-110,0;Enter MIN SPEED (%)...
				LITO	25
			ESBR
			SGLB	Drive/Get MIN SPEED	/2v,-120,120,-110,0;%.2f%%;
				LITO	25
			ESBR
			SGLB	Drive/ZERO SPD HYST	/3v,-120,120,0,100;Enter ZERO SPD HYST (%)...
				LITO	26
			ESBR
			SGLB	Drive/Get ZERO SPD HYST	/2v,-120,120,0,100;%.2f%%;
				LITO	26
			ESBR
			SGLB	Drive/ZERO SPEED LEVEL	/3v,-120,120,0,100;Enter ZERO SPEED LEVEL (%)...
				LITO	27
			ESBR
			SGLB	Drive/Get ZERO SPEED LEVEL	/2v,-120,120,0,100;%.2f%%;
				LITO	27
			ESBR
		ESTR
	ESBR
	SGLB	354602
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	General/Initialize
				LITO	31
			ESBR
			SGLB	Drive/Start	/:Link Method
				LITO	1828
			ESBR
			SGLB	Drive/Tag 463	/3v,-100,100,-100,100;Enter Tag 463 Data (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get Tag 463	/2v,-100,100;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/Tag 464	/3v,-100,100,-100,100;Enter Tag 464 Data (%)...
				LITO	4
			ESBR
			SGLB	Drive/Get Tag 464	/2v,-100,100;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/Tag 465	/3v,-100,100,-100,100;Enter Tag 465 Data (%)...
				LITO	6
			ESBR
			SGLB	Drive/Get Tag 465	/2v,-100,100;%.2f%%;
				LITO	6
			ESBR
			SGLB	Drive/Tag 466	/3v,-100,100,-100,100;Enter Tag 466 Data (%)...
				LITO	8
			ESBR
			SGLB	Drive/Get Tag 466	/2v,-100,100;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/Tag 467	/3v,-100,100,-100,100;Enter Tag 467 Data (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get Tag 467	/2v,-100,100;%.2f%%;
				LITO	10
			ESBR
			SGLB	Drive/Tag 468	/3v,-100,100,-100,100;Enter Tag 468 Data (%)...
				LITO	12
			ESBR
			SGLB	Drive/Get Tag 468	/2v,-100,100;%.2f%%;
				LITO	12
			ESBR
			SGLB	Drive/Tag 469	/3v,-100,100,-100,100;Enter Tag 469 Data (%)...
				LITO	14
			ESBR
			SGLB	Drive/Get Tag 469	/2v,-100,100;%.2f%%;
				LITO	14
			ESBR
			SGLB	Drive/Tag 470	/3v,-100,100,-100,100;Enter Tag 470 Data (%)...
				LITO	16
			ESBR
			SGLB	Drive/Get Tag 470	/2v,-100,100;%.2f%%;
				LITO	16
			ESBR
			SGLB	Drive/Tag 471	/3v,-100,100,-100,100;Enter Tag 471 Data (%)...
				LITO	18
			ESBR
			SGLB	Drive/Get Tag 471	/2v,-100,100;%.2f%%;
				LITO	18
			ESBR
			SGLB	Drive/Tag 472	/3v,-100,100,-100,100;Enter Tag 472 Data (%)...
				LITO	20
			ESBR
			SGLB	Drive/Get Tag 472	/2v,-100,100;%.2f%%;
				LITO	20
			ESBR
			SGLB	Drive/Tag 473	/3t,FALSE,TRUE;Enter Tag 473 Enable...
				LITO	22
			ESBR
			SGLB	Drive/Get Tag 473	/2t,FALSE,TRUE;
				LITO	22
			ESBR
			SGLB	Drive/Tag 474	/3t,FALSE,TRUE;Enter Tag 474 Enable...
				LITO	24
			ESBR
			SGLB	Drive/Get Tag 474	/2t,FALSE,TRUE;
				LITO	24
			ESBR
			SGLB	Drive/Tag 475	/3t,FALSE,TRUE;Enter Tag 475 Enable...
				LITO	26
			ESBR
			SGLB	Drive/Get Tag 475	/2t,FALSE,TRUE;
				LITO	26
			ESBR
			SGLB	Drive/Tag 476	/3t,FALSE,TRUE;Enter Tag 476 Enable...
				LITO	28
			ESBR
			SGLB	Drive/Get Tag 476	/2t,FALSE,TRUE;
				LITO	28
			ESBR
			SGLB	Drive/Tag 477	/3t,FALSE,TRUE;Enter Tag 477 Enable...
				LITO	30
			ESBR
			SGLB	Drive/Get Tag 477	/2t,FALSE,TRUE;
				LITO	30
			ESBR
			SGLB	Drive/Tag 478	/3t,FALSE,TRUE;Enter Tag 478 Enable...
				LITO	32
			ESBR
			SGLB	Drive/Get Tag 478	/2t,FALSE,TRUE;
				LITO	32
			ESBR
		ESTR
	ESBR
	SGLB	354556
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get TORQUE DEMAND	/2v,-200,200,-150,150;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/Get TORQUE FEEDBACK	/2v,-200,200,-150,150;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/Get CURRENT FEEDBACK	/2v,-200,200,-150,150;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/Get ACTUAL POS I LIM	/2v,-200,200,-150,150;%.2f%%;
				LITO	4
			ESBR
			SGLB	Drive/Get ACTUAL NEG I LIM	/2v,-200,200,-100,100;%.2f%%;
				LITO	5
			ESBR
			SGLB	Drive/Get AT CURRENT LIMIT	/2t,FALSE,TRUE;
				LITO	6
			ESBR
			SGLB	Drive/Get 1 / GAIN	/2u,0,255;
				LITO	7
			ESBR
			SGLB	Drive/POS TORQUE LIMIT	/3v,-200,200,-150,150;Enter POS TORQUE LIMIT (%)...
				LITO	8
			ESBR
			SGLB	Drive/Get POS TORQUE LIMIT	/2v,-200,200,-150,150;%.2f%%;
				LITO	8
			ESBR
			SGLB	Drive/NEG TORQUE LIMIT	/3v,-200,200,-150,150;Enter NEG TORQUE LIMIT (%)...
				LITO	9
			ESBR
			SGLB	Drive/Get NEG TORQUE LIMIT	/2v,-200,200,-150,150;%.2f%%;
				LITO	9
			ESBR
			SGLB	Drive/MAIN TORQUE LIM.	/3v,-200,200,0,150;Enter MAIN TORQUE LIM. (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get MAIN TORQUE LIM.	/2v,-200,200,0,150;%.2f%%;
				LITO	10
			ESBR
			SGLB	Drive/SYMETRIC TQ.LIM.	/3t,FALSE,TRUE;Enter SYMETRIC TQ.LIM....
				LITO	11
			ESBR
			SGLB	Drive/Get SYMETRIC TQ.LIM.	/2t,FALSE,TRUE;
				LITO	11
			ESBR
			SGLB	Drive/AUX TORQUE DMD	/3v,-150,150,-150,150;Enter AUX TORQUE DMD (%)...
				LITO	12
			ESBR
			SGLB	Drive/Get AUX TORQUE DMD	/2v,-150,150,-150,150;%.2f%%;
				LITO	12
			ESBR
			SGLB	Drive/TORQ.DMD.ISOLATE	/3t,FALSE,TRUE;Enter TORQ.DMD.ISOLATE...
				LITO	13
			ESBR
			SGLB	Drive/Get TORQ.DMD.ISOLATE	/2t,FALSE,TRUE;
				LITO	13
			ESBR
			SGLB	Drive/CURRENT LIMIT	/3v,-200,200,50,150;Enter CURRENT LIMIT (%)...
				LITO	14
			ESBR
			SGLB	Drive/Get CURRENT LIMIT	/2v,-200,200,50,150;%.2f%%;
				LITO	14
			ESBR
		ESTR
	ESBR
	SGLB	354563
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/CONTRAST	/3u,0,255;Enter CONTRAST...
				LITO	1
			ESBR
			SGLB	Drive/Get CONTRAST	/2u,0,255;
				LITO	1
			ESBR
			SGLB	Drive/FULL MENUS	/3t,FALSE,TRUE;Enter FULL MENUS...
				LITO	2
			ESBR
			SGLB	Drive/Get FULL MENUS	/2t,FALSE,TRUE;
				LITO	2
			ESBR
			SGLB	Drive/MENU DELAY	/3u,0,10000;Enter MENU DELAY...
				LITO	3
			ESBR
			SGLB	Drive/Get MENU DELAY	/2u,0,10000;
				LITO	3
			ESBR
			SGLB	Drive/DATA DELAY	/3v,-10000,10000,20,10000;Enter DATA DELAY...
				LITO	4
			ESBR
			SGLB	Drive/Get DATA DELAY	/2v,-10000,10000,20,10000;%.0f;
				LITO	4
			ESBR
		ESTR
	ESBR
	SGLB	354560
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get OUTPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/ENABLE	/3t,FALSE,TRUE;Enter ENABLE...
				LITO	2
			ESBR
			SGLB	Drive/Get ENABLE	/2t,FALSE,TRUE;
				LITO	2
			ESBR
			SGLB	Drive/INPUT	/3v,-300,300,-300,300;Enter INPUT (%)...
				LITO	3
			ESBR
			SGLB	Drive/Get INPUT	/2v,-300,300,-300,300;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/PROP.GAIN	/3v,-100,100,0,100;Enter PROP.GAIN...
				LITO	4
			ESBR
			SGLB	Drive/Get PROP.GAIN	/2v,-100,100,0,100;%.1f;
				LITO	4
			ESBR
			SGLB	Drive/INT.TIME CONST.	/3v,-100,100,0,100;Enter INT.TIME CONST. (Secs)...
				LITO	5
			ESBR
			SGLB	Drive/Get INT.TIME CONST.	/2v,-100,100,0,100;%.2fs;
				LITO	5
			ESBR
			SGLB	Drive/INT.DEFEAT	/3t,FALSE,TRUE;Enter INT.DEFEAT...
				LITO	6
			ESBR
			SGLB	Drive/Get INT.DEFEAT	/2t,FALSE,TRUE;
				LITO	6
			ESBR
			SGLB	Drive/DERIVATIVE TC	/3v,-10,10,0,10;Enter DERIVATIVE TC (Secs)...
				LITO	7
			ESBR
			SGLB	Drive/Get DERIVATIVE TC	/2v,-10,10,0,10;%.3fs;
				LITO	7
			ESBR
			SGLB	Drive/FILTER TC	/3v,-10,10,0,10;Enter FILTER TC (Secs)...
				LITO	8
			ESBR
			SGLB	Drive/Get FILTER TC	/2v,-10,10,0,10;%.3fs;
				LITO	8
			ESBR
			SGLB	Drive/POSITIVE LIMIT	/3v,-100,100,0,100;Enter POSITIVE LIMIT (%)...
				LITO	9
			ESBR
			SGLB	Drive/Get POSITIVE LIMIT	/2v,-100,100,0,100;%.2f%%;
				LITO	9
			ESBR
			SGLB	Drive/NEGATIVE LIMIT	/3v,-100,100,-100,0;Enter NEGATIVE LIMIT (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get NEGATIVE LIMIT	/2v,-100,100,-100,0;%.2f%%;
				LITO	10
			ESBR
			SGLB	Drive/O/P SCALER(TRIM)	/3v,-3,3,-3,3;Enter O/P SCALER(TRIM)...
				LITO	11
			ESBR
			SGLB	Drive/Get O/P SCALER(TRIM)	/2v,-3,3,-3,3;%.4f;
				LITO	11
			ESBR
			SGLB	Drive/MODE	/3u,0,4;Enter MODE...
				LITO	12
			ESBR
			SGLB	Drive/Get MODE	/2u,0,4;
				LITO	12
			ESBR
			SGLB	Drive/MIN PROFILE GAIN	/3v,-100,100,0,100;Enter MIN PROFILE GAIN (%)...
				LITO	13
			ESBR
			SGLB	Drive/Get MIN PROFILE GAIN	/2v,-100,100,0,100;%.2f%%;
				LITO	13
			ESBR
			SGLB	Drive/PROFILED GAIN	/3v,-100,100,0,100;Enter PROFILED GAIN...
				LITO	14
			ESBR
			SGLB	Drive/Get PROFILED GAIN	/2v,-100,100,0,100;%.1f;
				LITO	14
			ESBR
			SGLB	Drive/PROFILE INPUT	/3v,-100,100,0,100;Enter PROFILE INPUT (%)...
				LITO	15
			ESBR
			SGLB	Drive/Get PROFILE INPUT	/2v,-100,100,0,100;%.2f%%;
				LITO	15
			ESBR
			SGLB	Drive/PROFILE MININPUT	/3v,-100,100,0,100;Enter PROFILE MININPUT (%)...
				LITO	16
			ESBR
			SGLB	Drive/Get PROFILE MININPUT	/2v,-100,100,0,100;%.2f%%;
				LITO	16
			ESBR
			SGLB	Drive/CLAMPED	/3t,FALSE,TRUE;Enter CLAMPED...
				LITO	17
			ESBR
			SGLB	Drive/Get CLAMPED	/2t,FALSE,TRUE;
				LITO	17
			ESBR
		ESTR
	ESBR
	SGLB	354609
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get ERROR	/2v,-300,300,-300,300;%.2f%%;
				LITO	1
			ESBR
			SGLB	Drive/INPUT 1	/3v,-300,300,-300,300;Enter INPUT 1 (%)...
				LITO	2
			ESBR
			SGLB	Drive/Get INPUT 1	/2v,-300,300,-300,300;%.2f%%;
				LITO	2
			ESBR
			SGLB	Drive/INPUT 2	/3v,-300,300,-300,300;Enter INPUT 2 (%)...
				LITO	3
			ESBR
			SGLB	Drive/Get INPUT 2	/2v,-300,300,-300,300;%.2f%%;
				LITO	3
			ESBR
			SGLB	Drive/RATIO 1	/3v,-3,3,-3,3;Enter RATIO 1...
				LITO	4
			ESBR
			SGLB	Drive/Get RATIO 1	/2v,-3,3,-3,3;%.4f;
				LITO	4
			ESBR
			SGLB	Drive/RATIO 2	/3v,-3,3,-3,3;Enter RATIO 2...
				LITO	5
			ESBR
			SGLB	Drive/Get RATIO 2	/2v,-3,3,-3,3;%.4f;
				LITO	5
			ESBR
			SGLB	Drive/SIGN 1	/3t,NEG,POS;Enter SIGN 1...
				LITO	6
			ESBR
			SGLB	Drive/Get SIGN 1	/2t,NEG,POS;
				LITO	6
			ESBR
			SGLB	Drive/SIGN 2	/3t,NEG,POS;Enter SIGN 2...
				LITO	7
			ESBR
			SGLB	Drive/Get SIGN 2	/2t,NEG,POS;
				LITO	7
			ESBR
			SGLB	Drive/DIVIDER 1	/3v,-3,3,-3,3;Enter DIVIDER 1...
				LITO	8
			ESBR
			SGLB	Drive/Get DIVIDER 1	/2v,-3,3,-3,3;%.4f;
				LITO	8
			ESBR
			SGLB	Drive/DIVIDER 2	/3v,-3,3,-3,3;Enter DIVIDER 2...
				LITO	9
			ESBR
			SGLB	Drive/Get DIVIDER 2	/2v,-3,3,-3,3;%.4f;
				LITO	9
			ESBR
			SGLB	Drive/LIMIT	/3v,-300,300,-300,300;Enter LIMIT (%)...
				LITO	10
			ESBR
			SGLB	Drive/Get LIMIT	/2v,-300,300,-300,300;%.2f%%;
				LITO	10
			ESBR
		ESTR
	ESBR
	SGLB	354607
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Id PROP GAIN	/3u,0,32767;Enter Id PROP GAIN...
				LITO	1
			ESBR
			SGLB	Drive/Get Id PROP GAIN	/2u,0,32767;
				LITO	1
			ESBR
			SGLB	Drive/Id INT GAIN	/3u,0,32767;Enter Id INT GAIN...
				LITO	2
			ESBR
			SGLB	Drive/Get Id INT GAIN	/2u,0,32767;
				LITO	2
			ESBR
			SGLB	Drive/MAX Id DEMAND	/3u,0,10000;Enter MAX Id DEMAND...
				LITO	3
			ESBR
			SGLB	Drive/Get MAX Id DEMAND	/2u,0,10000;
				LITO	3
			ESBR
			SGLB	Drive/MIN Id DEMAND	/3v,-5000,5000,-5000,-1;Enter MIN Id DEMAND...
				LITO	4
			ESBR
			SGLB	Drive/Get MIN Id DEMAND	/2v,-5000,5000,-5000,-1;%.0f;
				LITO	4
			ESBR
			SGLB	Drive/MAX Id INTEGRAL	/3u,0,10000;Enter MAX Id INTEGRAL...
				LITO	5
			ESBR
			SGLB	Drive/Get MAX Id INTEGRAL	/2u,0,10000;
				LITO	5
			ESBR
			SGLB	Drive/MIN Id INTEGRAL	/3v,-5000,5000,-5000,0;Enter MIN Id INTEGRAL...
				LITO	6
			ESBR
			SGLB	Drive/Get MIN Id INTEGRAL	/2v,-5000,5000,-5000,0;%.0f;
				LITO	6
			ESBR
			SGLB	Drive/Iq INT GAIN	/3u,0,32767;Enter Iq INT GAIN...
				LITO	7
			ESBR
			SGLB	Drive/Get Iq INT GAIN	/2u,0,32767;
				LITO	7
			ESBR
			SGLB	Drive/MAX Iq INTEGRAL	/3u,0,5000;Enter MAX Iq INTEGRAL...
				LITO	8
			ESBR
			SGLB	Drive/Get MAX Iq INTEGRAL	/2u,0,5000;
				LITO	8
			ESBR
			SGLB	Drive/MIN Iq INTEGRAL	/3v,-5000,5000,-5000,0;Enter MIN Iq INTEGRAL...
				LITO	9
			ESBR
			SGLB	Drive/Get MIN Iq INTEGRAL	/2v,-5000,5000,-5000,0;%.0f;
				LITO	9
			ESBR
			SGLB	Drive/MAX Id HI WORD	/3v,-1,1,-1,0;Enter MAX Id HI WORD...
				LITO	10
			ESBR
			SGLB	Drive/Get MAX Id HI WORD	/2v,-1,1,-1,0;%.0f;
				LITO	10
			ESBR
			SGLB	Drive/MIN Id HI WORD	/3v,-1,1,-1,0;Enter MIN Id HI WORD...
				LITO	11
			ESBR
			SGLB	Drive/Get MIN Id HI WORD	/2v,-1,1,-1,0;%.0f;
				LITO	11
			ESBR
			SGLB	Drive/Get 584S CHASSIS	/2t,FALSE,TRUE;
				LITO	12
			ESBR
			SGLB	Drive/BYPASS PASSWORD	/3t,FALSE,TRUE;Enter BYPASS PASSWORD...
				LITO	13
			ESBR
			SGLB	Drive/Get BYPASS PASSWORD	/2t,FALSE,TRUE;
				LITO	13
			ESBR
			SGLB	Drive/SKIP CO-PRO INIT	/3t,FALSE,TRUE;Enter SKIP CO-PRO INIT...
				LITO	14
			ESBR
			SGLB	Drive/Get SKIP CO-PRO INIT	/2t,FALSE,TRUE;
				LITO	14
			ESBR
			SGLB	Drive/BRAKE THRESHOLD	/3u,0,1023;Enter BRAKE THRESHOLD...
				LITO	15
			ESBR
			SGLB	Drive/Get BRAKE THRESHOLD	/2u,0,1023;
				LITO	15
			ESBR
			SGLB	Drive/MODN INDEX	/3u,0,12000;Enter MODN INDEX...
				LITO	16
			ESBR
			SGLB	Drive/Get MODN INDEX	/2u,0,12000;
				LITO	16
			ESBR
			SGLB	Drive/AD POS THRESHOLD	/3u,0,100;Enter AD POS THRESHOLD...
				LITO	17
			ESBR
			SGLB	Drive/Get AD POS THRESHOLD	/2u,0,100;
				LITO	17
			ESBR
			SGLB	Drive/AD NEG THRESHOLD	/3u,0,100;Enter AD NEG THRESHOLD...
				LITO	18
			ESBR
			SGLB	Drive/Get AD NEG THRESHOLD	/2u,0,100;
				LITO	18
			ESBR
			SGLB	Drive/Get DRIVE STATUS	/2t,FALSE,TRUE;
				LITO	19
			ESBR
			SGLB	Drive/Get DRIVE RATING RMS	/2v,-3000,3000,0.1,3000;%.1fA;
				LITO	20
			ESBR
			SGLB	Drive/Get MID VOLTS	/2t,FALSE,TRUE;
				LITO	21
			ESBR
			SGLB	Drive/Get CHASSIS TYPE	/2u,584,587;
				LITO	22
			ESBR
			SGLB	Drive/RESET VEC VARS	/3t,FALSE,TRUE;Enter RESET VEC VARS...
				LITO	23
			ESBR
			SGLB	Drive/Get RESET VEC VARS	/2t,FALSE,TRUE;
				LITO	23
			ESBR
			SGLB	Drive/Get RESET EAT	/2t,FALSE,TRUE;
				LITO	24
			ESBR
			SGLB	Drive/MIN MMI CYCLE TM	/3u,0,30000;Enter MIN MMI CYCLE TM...
				LITO	25
			ESBR
			SGLB	Drive/Get MIN MMI CYCLE TM	/2u,0,30000;
				LITO	25
			ESBR
			SGLB	Drive/MAX MMI CYCLE TM	/3u,0,30000;Enter MAX MMI CYCLE TM...
				LITO	26
			ESBR
			SGLB	Drive/Get MAX MMI CYCLE TM	/2u,0,30000;
				LITO	26
			ESBR
			SGLB	Drive/Get CYCLE TIME	/2u,0,10000;
				LITO	27
			ESBR
			SGLB	Drive/Get SYS TIME	/2x;0x%4.4X;
				LITO	28
			ESBR
			SGLB	Drive/Get ENCODER COUNTER	/2v,-10000,10000,-10000,10000;%.0f;
				LITO	29
			ESBR
			SGLB	Drive/SPD.FBK. TC	/3v,-30,30,0,30;Enter SPD.FBK. TC (Secs)...
				LITO	30
			ESBR
			SGLB	Drive/Get SPD.FBK. TC	/2v,-30,30,0,30;%.3fs;
				LITO	30
			ESBR
			SGLB	Drive/TORQUE.FBK.TC	/3v,-30,30,0,30;Enter TORQUE.FBK.TC (Secs)...
				LITO	31
			ESBR
			SGLB	Drive/Get TORQUE.FBK.TC	/2v,-30,30,0,30;%.3fs;
				LITO	31
			ESBR
			SGLB	Drive/P3 TAG LIST TC	/3v,-30,30,0,30;Enter P3 TAG LIST TC (Secs)...
				LITO	32
			ESBR
			SGLB	Drive/Get P3 TAG LIST TC	/2v,-30,30,0,30;%.3fs;
				LITO	32
			ESBR
			SGLB	Drive/IFB ADJUST	/3v,-150,150,50,150;Enter IFB ADJUST (%)...
				LITO	33
			ESBR
			SGLB	Drive/Get IFB ADJUST	/2v,-150,150,50,150;%.1f%%;
				LITO	33
			ESBR
			SGLB	Drive/TOTAL TRIP COUNT	/3x;Enter TOTAL TRIP COUNT...
				LITO	34
			ESBR
			SGLB	Drive/Get TOTAL TRIP COUNT	/2x;0x%4.4X;
				LITO	34
			ESBR
			SGLB	Drive/Get SYSTEM RESET	/2t,FALSE,TRUE;
				LITO	35
			ESBR
			SGLB	Drive/Get SELECT FUNCTION	/2u,0,9;
				LITO	36
			ESBR
			SGLB	Drive/SPEED PERIOD	/3u,2,-1;Enter SPEED PERIOD...
				LITO	37
			ESBR
			SGLB	Drive/Get SPEED PERIOD	/2u,2,-1;
				LITO	37
			ESBR
			SGLB	Drive/SPEED AMPLITUDE	/3u,0,30000;Enter SPEED AMPLITUDE...
				LITO	38
			ESBR
			SGLB	Drive/Get SPEED AMPLITUDE	/2u,0,30000;
				LITO	38
			ESBR
			SGLB	Drive/SPEED OFFSET	/3v,-11000,11000,-11000,11000;Enter SPEED OFFSET...
				LITO	39
			ESBR
			SGLB	Drive/Get SPEED OFFSET	/2v,-11000,11000,-11000,11000;%.0f;
				LITO	39
			ESBR
			SGLB	Drive/CURRENT PERIOD	/3v,-10000,10000,2,10000;Enter CURRENT PERIOD...
				LITO	40
			ESBR
			SGLB	Drive/Get CURRENT PERIOD	/2v,-10000,10000,2,10000;%.0f;
				LITO	40
			ESBR
			SGLB	Drive/CURR AMPLITUDE	/3u,0,5000;Enter CURR AMPLITUDE...
				LITO	41
			ESBR
			SGLB	Drive/Get CURR AMPLITUDE	/2u,0,5000;
				LITO	41
			ESBR
			SGLB	Drive/CURRENT OFFSET	/3v,-5000,5000,-5000,5000;Enter CURRENT OFFSET...
				LITO	42
			ESBR
			SGLB	Drive/Get CURRENT OFFSET	/2v,-5000,5000,-5000,5000;%.0f;
				LITO	42
			ESBR
		ESTR
	ESBR
	SGLB	354558
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Drive/Get ENCODER LINES	/2u,0,8000;
				LITO	1
			ESBR
			SGLB	Drive/MAX SPEED RPM	/3v,-32000,32000,0,32000;Enter MAX SPEED RPM (RPM)...
				LITO	2
			ESBR
			SGLB	Drive/Get MAX SPEED RPM	/2v,-32000,32000,0,32000;%.0fRPM;
				LITO	2
			ESBR
			SGLB	Drive/Get BASE FREQUENCY	/2v,-400,400,0.1,400;%.1fHz;
				LITO	3
			ESBR
			SGLB	Drive/MOTOR VOLTS	/3v,-1000,1000,0,1000;Enter MOTOR VOLTS (Volts)...
				LITO	4
			ESBR
			SGLB	Drive/Get MOTOR VOLTS	/2v,-1000,1000,0,1000;%.0fV;
				LITO	4
			ESBR
			SGLB	Drive/Get MOTOR RATING RMS	/2v,-3000,3000,0.1,3000;%.1fA;
				LITO	5
			ESBR
			SGLB	Drive/Get NO.OF POLES	/2v,-50,50,2,50;%.0f;
				LITO	6
			ESBR
			SGLB	Drive/Get NAMEPLATE RPM	/2v,-32000,32000,0,32000;%.0fRPM;
				LITO	7
			ESBR
		ESTR
	ESBR
	SGLB	354157
		STRE
			SORD	0
				CLAS	354008
			ESBR
			SGLB	Utility/Event
			ESBR
			SGLB	Utility/Trigger
			ESBR
			SGLB	Utility/Get Next
			ESBR
			SGLB	Utility/Debug	/1
			ESBR
			SGLB	Utility/Get Address Matches	/2u2
			ESBR
			SGLB	Utility/Get CRC Errors	/2u2
			ESBR
			SGLB	Utility/Get Overruns	/2u2
			ESBR
			SGLB	Utility/Get Fragments	/2u2
			ESBR
			SGLB	Utility/Get State	/4u,1,3000;Enter address|e,Unknown,Halted,No Configuration,L Error,H Error,Selt-Test Failure,Abort,OK,Network Warning,Network Failure
			ESBR
			SGLB	Utility/Filter
			ESBR
		ESTR
	ESBR
	SGLB	354538
		STRE
			SORD	0
				CLAS	354044
			ESBR
			SGLB	General/Initialize
			ESBR
			SGLB	Vector/Read Tag
			ESBR
			SGLB	Vector/Write Tag
			ESBR
			SGLB	Vector/Get Tag Info	/4u,0,1023;Enter Tag Number|l
			ESBR
		ESTR
	ESBR
ESTR
